Low odor acrylic monomer SW107
Section 1   IDENTIFICATION OF SUBSTANCE AND OF THE COMPANY
[bookmark: _GoBack]Product Name: Low odor acrylic monomer SW107
Company Name: Guangzhou Wangsan Technology CO.,Ltd. . 
Tel: +86-20-82562016       Fax: +86-20-31078112
E-mail address: admin@gzwangsanchem.com
Address: NO.1 301 Hong bafang investment BLDG1.Guanchong villageShiqi town, Panyu district,Guangzhou city,Guangdong Province,China
SECTION 2 - COMPOSITION, INFORMATION ON INGREDIENTS
Low odor acrylic monomer SW107
CAS No.: - 
EINECS : -
Purity: 100%
SECTION 3 - HAZARDS IDENTIFICATION
non-hazardous material
SECTION 4 - FIRST AID MEASURES Ingestion:
If swallowed, call a physician immediately. Only induce vomiting at the instruction of a physician. Never give anything by mouth to an
unconscious person.
Skin contact:
Wash immediately with soap and a lot of water.
Eye contact:
Rinse immediately with plenty of water for at least 15 minutes. Obtain medical attention immediately.
Inhalation:
Remove to fresh air. If breathing is difficult, give oxygen. Obtain medical advice if there are persistent symptoms.


SECTION 5 - FIRE FIGHTING MEASURES Fire Extinguishing Media:
Foam, Carbon dioxide，chemical dry powder
Hazards that may be encountered when extinguishing a fire: 
1. The spillage should be stopped before extinguishing the fire, if it cannot be stopped and there is no hazardous material around, let the spillage burn out; 
2. If the fire is extinguished without stopping the spillage, the vapour may form an explosive mixture with the air and ignite again.
Special protective equipment for firefighters: full face shield, respiratory protection, protective gloves, protective clothing.
SECTION 6 - ACCIDENTAL RELEASE MEASURES
Personal precautions:
Limit duration and extent of exposure. Avoid contacdt with the skin and the eyes. For personal protection see section 8. Ensure adequate ventilation.   Evacuate personnel to safe areas. Keep people away from and upwind of  spill/leak.
Environmental Precautions:
Must not get into the soil, sewerage systems and suface water. In the event of Contamination, notify the responsible authorities.
Methods for cleaning up:
Soak up with inert absorbent material(e.g. sand, silica gel, acid binder, universal binder, sawdust).


SECTION 7 - HANDLING and STORAGE Handling:
Handle and open container with care. Avoid contact with skin and eyes. Provide     emergency eye-rinse and shower for entire body. Do not eat or drink near the area of application. Use only in a well-ventilated room. Use exhauster devices. Limit
duration and extent of exposure. Keep away from heat and sources of ignition. Avoid overheating. Do not smoke.
Storage:
Keep container tightly closed in a dry and well-ventilated place. Store in the original container at room temperature. Containers of precious steel(316), polyethylene,
polypropylene. Use PTFE seals. Keep away from oxidizing agents. Keep away from food, drink and animal feeding stuffs. Product must be kept and stored in such a
way that it does not present a hazard to people’s health and the environment.

SECTION 8 - EXPOSURE CONTROLS, PERSONAL PROTECTION Engineering Measures:
Utilize a closed system process where feasible.
Where this material is not used in a closed system, good enclosure and local exhaust ventilation should be provided to control exposure.
Respiratory protection:
This should be achieved by a good general extraction and –if practically feasible-by the use of a local exhaust ventilation.
Eye protection:
Face shield or goggles
Tightly fitting safety goggles
Skin Protection:
Wear closed work/protective clothing. When working outside a closed system, additionally put on aprons made of polyethylene.

	
	
	OELs（8-hour base period）
	OELs（15min）

	Country
	Material
	ppm
	mg/m³
	ppm
	mg/m³
	Note

	China
	SW107
	1
	5
	2
	10
	No skin contact


Hand Protection:
Protective gloves
Additional advice:
Use only in area provided with appropriate exhaust ventilation.
SECTION 9 - PHYSICAL AND CHEMICAL PROPERTIES
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Material safety data sheet
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Appearance
Colorless clear liquid

Color APHA
25MAX
Odor
Slightly irritating

TG
65

Viscosity
5-10

Melting point
≤60
Boiling point
200.32℃

Flash point
101℃

Water absorption
2.4

vapor pressure（20℃）
0.1hpa（21.41℃）

Density
1098.05 kg/m³（30.1℃）

Solubility
1000g/L(200℃）

Octanol/water（log po/w）
0.17（25
Dynamic Viscosity
11.168 mPas(25℃）
4
Surface tension
25.65mN/m（16℃）

SECTION 10 - STABILITY AND REACTIVITY Stability: Stable
Material to Avoid: Keep away from oxidizing agents in order to avoid exothermic reactions.
SECTION 11 - TOXICOLOGICAL INFORMATION Toxicological Tests
Other Information: No data available
Experiences form usage: No data available
General Remarks: Other dangerous properties cannot be excluded. Harmful by inhalation, in contact with skin and if swallowed.
SECTION 12 - ECOLOGICAL INFORMATION PBT/vPvB assessment：No PBT/vPvB
Endocrine disrupting properties: No endocrine disrupting properties

SECTION 13 - DISPOSAL CONSIDERATIONS
Recommendation for The Product:
Do not discharge product unmonitored into the environment. Must be disposed of as hazardous waste according to the national legal
regulations. Can be incinerated when in compliance with local regulations.
Recommendations for Packing:
Packaging that cannot be cleaned should be disposed of like the product.
Recommended Cleaning Agent
Industrial cleaning agent
Additional Advice:
The allocation of waste key numbers must be conducted according to specific industrial sectors and processes.

SECTION 14 - TRANSPORT INFORMATION 
	
	Land transport
（ADR/RID)
	River transport
(ADN)
	Sea transport
(MDG)
	Air transport
(ICAO/IATA)

	UN No.
	UN2922
	UN2922
	UN2922
	UN2922

	 shipping name
	corrosive liquids.toxic
	corrosive liquids.toxic
	corrosive liquids.toxic
	corrosive liquids.toxic

	 Hazard Classification
	8/6.1
	8/6.1
	8/6.1
	8/6.1

	Packaging category
	Ⅲ
	Ⅲ
	Ⅱ
	Ⅲ

	Marine pollutants (Yes/No)
	No
	No
	No
	No

	Bulk Transportation Reference IBC Rules
	IBC02
	IBC02
	IBC02
	IBC02



SECTION 15 - REGULATORY INFORMATION 
Specific safety, health and environmental regulations for the substance or mixture 

Authorization Information
not applicable

Restricted information
not applicable

Other EU regulations
Trained personnel only

Chemical safety assessed
SECTION 16 - ADDITIONAL INFORMATION
The information above is believed to be accurate and represents the best
information currently available to us. However, we make no warranty of merchantability or any other warranty, express or implied, with respect to such information, and we
assume no liability resulting from its use. Users should make their own investigations to determine the suitability of the information for their particular purposes. In no way shall  the company be liable for any claims, losses, or damages of any third party or for lost    profits or any special, indirect, incidental, consequential or exemplary damages,
howsoever arising, even if the company has been advised of the possibility of such damages.
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GUANGZHOU WANGSAN TECHNOLOGY CO.,LTD




