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MATERIAL SAFETY DATA SHEET
Product: PALLET COATING 2706 H
Date: 29/07/2026
1. IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING
Product identifier:  Coating 2706 H
CAS number: Not available
Use of substance/mixture: Water-based coating for interior wooden products
Supplier: Binh Thanh Chemical Glue Production & Trading Co., Ltd (BT Chem)
Address: Group 4, Binh Phuoc B Quarter, An Phu Ward, Ho Chi Minh City, Vietnam
Phone: +84 274 3789 99 (1-7)
Email: lab@btchem.com.vn
Emergency phone: +84 274 3789 993
2. HAZARDS IDENTIFICATION
GHS Classification: Not classified as hazardous under GHS criteria for this product.
Label elements:
  Hazard pictograms: Product does not require a hazard warning label under GHS criteria.
  GHS label: Product does not require a hazard warning label under GHS criteria.
  Hazard statements: Not applicable
  Precautionary statements: Not applicable
  Other hazards: Not applicable
3. COMPOSITION/INFORMATION ON INGREDIENTS
	Component
	CAS No.
	% by weight

	Acrylic resin
	n/a
	70–90

	Coalescent
	25265-77-4
	1–2

	Extender powder
	n/a
	5–10

	De-ionized water
	7732-18-5
	5–10



4. FIRST AID MEASURES
Description of first aid measures:
Eye contact: Rinse cautiously with water for several minutes. Remove contact lenses if present and easy to do. Continue rinsing. Seek medical attention if pain, blinking, or redness persists.
Skin contact: Wash with plenty of soap and water. If skin irritation or rash occurs: seek medical advice/attention. Wash contaminated clothing before reuse.
Inhalation: If symptoms appear: move to fresh air and ventilate the suspected area.
Ingestion: Do NOT induce vomiting. If vomiting occurs spontaneously, keep head lower than hips to avoid inhalation. Transport to nearest medical facility for further treatment.
5. FIREFIGHTING MEASURES
Suitable extinguishing media: Dry sand, CO₂, foam, dry powder.
Unsuitable extinguishing media: Strong water jet.
Special hazards: Hazardous combustion products: Carbon dioxide, carbon monoxide, toxic pyrolysis products.
Protective equipment for firefighters: Use suitable breathing apparatus, protective clothing, rubber boots, rubber gloves.
Additional information: Use strong water spray to protect personnel and cool endangered containers. Move undamaged containers away from hazard area immediately if safe to do so.
6. ACCIDENTAL RELEASE MEASURES
Personal precautions: See section 8 for PPE. Wear protective clothing and gloves.
Emergency procedures: Absorb with inert absorbent material (e.g., sand, sawdust, universal binder, silica gel).
Environmental precautions: Avoid discharge into the environment.
Methods for containment/cleaning: Clean up spills as soon as possible using absorbent material. Collect all waste in suitable labeled containers and dispose of according to local regulations.
7. HANDLING AND STORAGE
Handling:
  • Wash hands thoroughly after handling.
  • Ensure good ventilation of the work area (use local exhaust ventilation if necessary).
  • During handling and use, comply with occupational exposure limits as directed.
Storage:
  • Store in a cool, dry, well-ventilated area.
  • Keep container tightly closed when not in use.
  • Keep away from heat sources and direct sunlight.
  • Storage temperature: 5°C to 35°C.
  • Reason: To ensure product quality.
8. EXPOSURE CONTROLS/PERSONAL PROTECTION
Exposure limits: No established values.
Engineering measures: Engineering controls are generally not required if good hygiene practices are followed.
Respiratory protection: If inhalation risk exists, use organic vapor respirator.
Eye protection: Wear chemical splash goggles or full face shield. Prepare eyewash station and emergency shower near work area.
Skin protection: Wear impermeable gloves and protective clothing. Replace gloves immediately if torn or damaged.
General: Do not eat, drink, or smoke at the workplace. Wash hands and face before eating, drinking, or smoking.
9. PHYSICAL AND CHEMICAL PROPERTIES
	Property
	Value

	Physical state
	Liquid

	Color
	As per sample

	Odor
	Mild characteristic odor

	pH
	7–9

	Melting point
	No data

	Freezing point
	No data

	Boiling point
	No data

	Flammability
	No data

	Auto-ignition temperature
	No data

	Decomposition temperature
	No data

	Vapor pressure
	No data

	Relative vapor density
	No data

	Relative density
	No data

	Solubility
	No data

	Viscosity
	No data

	Explosive properties
	No data

	Oxidizing properties
	No data

	Explosion limits
	No data



10. STABILITY AND REACTIVITY
Stability: Stable under normal (room temperature) conditions and recommended storage (see Section 7).
Conditions to avoid: Avoid heat and open flames.
Materials to avoid: Avoid contact with strong oxidizing agents, strong alkalis, and strong acids.
Hazardous decomposition products: A complex mixture of airborne solids, liquids, and gases including carbon monoxide, carbon dioxide, and other organic compounds will be released upon combustion or thermal/oxidative decomposition.
11. TOXICOLOGICAL INFORMATION
	Endpoint
	Classification

	Acute skin irritation
	Not classified

	Acute eye irritation
	Not classified

	Respiratory sensitization
	Not classified

	Respiratory sensitizer
	Not classified



Symptoms related to physical, chemical, and toxicological properties:
  Ingestion: No data available
  Skin contact: Non-irritating
  Inhalation: No data available
12. ECOLOGICAL INFORMATION
This substance is not classified as hazardous to the environment.
	Parameter
	Value

	Ecotoxicity
	None

	Bioaccumulation potential
	None

	Persistence and degradability
	None

	Mobility in soil
	None

	Other adverse effects - Ozone depletion
	None



13. DISPOSAL CONSIDERATIONS
Regional legislation (waste): Disposal must be carried out in accordance with official regulations.
Waste treatment methods: Recycling is preferred over disposal or incineration. Do not pour into drains. Dispose of this material and its container at hazardous or special waste collection points. Collect spill liquid into absorbent material, e.g., sand/soil.
Waste disposal recommendation: Dispose of contents/container to...
Ecology — waste material: Empty containers should be collected for recycling, recovery, or disposal per local regulations.
14. TRANSPORT INFORMATION
Domestic transport: Not classified as dangerous goods under transport regulations.
Sea transport (IMDG): Not classified as dangerous goods under transport regulations.
Air transport (IATA/ICAO): Not classified as dangerous goods under transport regulations.
15. REGULATORY INFORMATION
Registration status:
  EU Regulations:
    • Does not contain REACH substances with Annex XVII restrictions
    • Does not contain substances on the REACH Candidate List
    • Does not contain REACH Annex XIV substances
  National regulations: No additional information available.
Hazard classification by country: The product does not contain hazardous substances such as: toxic heavy metals, free formaldehyde, azo compounds, phthalates, benzene, etc., complying with REACH, EN.71-3 (Europe) and CPSIA, ASTM (USA) standards.
16. OTHER INFORMATION
Preparation date: 07/07/2026
Data sources:
The information above exclusively describes the safety requirements of the product and is based on our current knowledge. This information is intended to advise you on the safe handling of the product named in this safety data sheet for storage, processing, transport, and disposal.
The information cannot be transferred to other products. In case of mixing with other products or processing, the information in this safety data sheet does not necessarily apply to the new material.
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