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MATERIAL SAFETY DATA SHEET
Product: PRESERVATIVE OIL 1009 H
Date: 05/10/2026
1. IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING
Product identifier: PRESERVATIVE OIL 1009 H
CAS number: Not available
Use of substance/mixture: Water-based preservative oil for wooden product surfaces
Supplier: Binh Thanh Chemical Glue Production & Trading Co., Ltd (BT Chem)
Address: Group 4, Binh Phuoc B Quarter, An Phu Ward, Ho Chi Minh City, Vietnam
Phone: +84 274 3789 99 (1-7)
Email: lab@btchem.com.vn
Emergency phone: +84 274 3789 993
2. HAZARDS IDENTIFICATION
GHS Classification: Not classified as hazardous under GHS criteria for this product.
Label elements:
Hazard pictograms: Product does not require a hazard warning label under GHS criteria.
GHS label: Product does not require a hazard warning label under GHS criteria.
Hazard statements: Not applicable
Precautionary statements: Not applicable
Other hazards: Not applicable
3. COMPOSITION/INFORMATION ON INGREDIENTS
	Component
	CAS No.
	% by weight

	Water-based polymer resin (aqueous dispersion)
	Not available (mixture)
	60 – 70

	Glycerol
	56-81-5
	10 – 15

	Deionised water
	7732-18-5
	5 – 10

	Monoethylene glycol
	107-21-1
	5 – 10

	Amorphous silica (matting agent)
	7631-86-9
	2 – 3

	Additives (defoamer, wetting agent, surface additive, preservative, rheology modifier)
	Not available
	< 2



4. FIRST AID MEASURES
Eye contact: Rinse cautiously with water for several minutes. Remove contact lenses if present and easy to do. Continue rinsing. Seek medical attention if pain persists.
Skin contact: Wash with plenty of soap and water. If skin irritation or rash occurs: seek medical advice. Wash contaminated clothing before reuse.
Inhalation: If symptoms appear: move to fresh air and ventilate the suspected area.
Ingestion: Do NOT induce vomiting. If vomiting occurs spontaneously, keep head lower than hips. Transport to nearest medical facility.
5. FIREFIGHTING MEASURES
Suitable extinguishing media: Dry sand, CO₂, foam, dry powder.
Unsuitable extinguishing media: Strong water jet.
Hazardous combustion products: CO₂, CO, toxic pyrolysis products.
Firefighter protection: Use breathing apparatus, protective clothing, rubber boots, gloves.
6. ACCIDENTAL RELEASE MEASURES
Personal precautions: See section 8 for PPE. Wear protective clothing and gloves.
Emergency procedures: Absorb with inert absorbent material (sand, sawdust, silica gel).
Environmental precautions: Avoid discharge into the environment.
Cleanup methods: Clean up spills immediately using absorbent material. Collect waste in labeled containers per local regulations.
7. HANDLING AND STORAGE
Handling: Wash hands after handling. Ensure good ventilation. Comply with occupational exposure limits.
Storage: Cool, dry, well-ventilated area. Keep container closed. Keep away from heat/sunlight. Storage temperature: 5°C–35°C.
8. EXPOSURE CONTROLS/PERSONAL PROTECTION
Exposure limits: Not established.
Respiratory protection: Use organic vapor respirator if inhalation risk exists.
Eye protection: Wear splash goggles. Eyewash station nearby.
Skin protection: Wear impermeable gloves, protective clothing.
General: No eating/drinking/smoking at workplace.
9. PHYSICAL AND CHEMICAL PROPERTIES
	Property
	Value

	Physical state
	Liquid

	Color
	Milky white

	Odor
	Mild characteristic odor

	pH
	No data

	Melting point
	No data

	Boiling point
	No data

	Flammability
	Not flammable

	Vapor pressure
	No data

	Relative density
	No data

	Solubility
	Dispersible in water

	Viscosity
	No data



10. STABILITY AND REACTIVITY
Stability: Stable under normal conditions and recommended storage.
Conditions to avoid: Heat and open flames.
Materials to avoid: Strong oxidizing agents, strong alkalis, strong acids.
Hazardous decomposition: CO, CO₂, and other organic compounds upon combustion or thermal decomposition.
11. TOXICOLOGICAL INFORMATION
	Endpoint
	Classification

	Acute skin irritation
	Not classified

	Acute eye irritation
	Not classified

	Respiratory sensitization
	Not classified



12. ECOLOGICAL INFORMATION
Not classified as hazardous to the environment.
	Parameter
	Value

	Ecotoxicity
	None

	Bioaccumulation
	None

	Persistence/degradability
	None



13. DISPOSAL CONSIDERATIONS
Dispose in accordance with official regulations. Do not pour into drains.
14. TRANSPORT INFORMATION
Domestic/Sea/Air: Not classified as dangerous goods under transport regulations.
15. REGULATORY INFORMATION
EU Regulations: Does not contain restricted REACH Annex XVII substances, REACH Candidate List substances, or REACH Annex XIV substances.
Product does not contain toxic heavy metals, free formaldehyde, azo compounds, phthalates, benzene. Complies with REACH, EN.71-3 (Europe), and CPSIA, ASTM (USA).
16. OTHER INFORMATION
Preparation date: 05/10/2026
The information describes safety requirements based on current knowledge. It is intended for safe handling, storage, processing, transport, and disposal of the product. Information does not necessarily apply to mixtures or processed materials.
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