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MATERIAL SAFETY DATA SHEET
Product: PRESERVATIVE OIL 1209DM
Date: 05/10/2026
1. IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING
Product identifier: PRESERVATIVE OIL 1209DM
CAS number: Not available
Use of substance/mixture: Solvent-based preservative oil for wooden product surfaces
Supplier: Binh Thanh Chemical Glue Production & Trading Co., Ltd (BT Chem)
Address: Group 4, Binh Phuoc B Quarter, An Phu Ward, Ho Chi Minh City, Vietnam
Phone: +84 274 3789 99 (1-7)
Email: lab@btchem.com.vn
Emergency phone: +84 274 3789 993
2. HAZARDS IDENTIFICATION
GHS Classification: Flammable liquid (Flam. Liq. 3, H226); may cause cancer (Carc. 1B, H350); may damage the unborn child (Repr. 1B, H360D); may cause an allergic skin reaction (Skin Sens. 1, H317); may cause drowsiness or dizziness (STOT SE 3, H336)
Label elements:
Hazard pictograms: GHS02 (flame) · GHS07 (exclamation mark) · GHS08 (health hazard)
GHS label: DANGER
Hazard statements: H226 – Flammable liquid and vapour; H350 – May cause cancer; H360D – May damage the unborn child; H317 – May cause an allergic skin reaction; H336 – May cause drowsiness or dizziness
Precautionary statements: P210 – Keep away from heat/sparks/open flames; P260 – Do not breathe vapour/spray; P280 – Wear protective gloves/eye protection/protective clothing; P302+P352 – IF ON SKIN: wash with plenty of soap and water; P308+P313 – IF exposed or concerned: get medical advice; P403+P235 – Store in a well-ventilated place. Keep cool
Other hazards: Solvent vapours are heavier than air and may travel to ignition sources and flash back
3. COMPOSITION/INFORMATION ON INGREDIENTS
	Component
	CAS No.
	% by weight

	Long-oil alkyd resin
	Not available (mixture)
	40 – 50

	Hydrocarbon solvent (petroleum fraction)
	64742-88-7
	20 – 30

	Dibasic ester solvent
	627-93-0 / 1119-40-0 / 106-65-0
	20 – 30

	Amorphous silica (matting agent)
	7631-86-9
	2 – 4

	Thickener (organoclay/xylene)
	1330-20-7
	2 – 3

	Driers (cobalt and cobalt-free metal carboxylates)
	136-52-7
	< 1

	Anti-skinning agent (oxime)
	96-29-7
	< 1

	Other additives (defoamer, surface additive, fungicide)
	Not available
	< 1



4. FIRST AID MEASURES
Eye contact: Rinse cautiously with water for several minutes. Remove contact lenses if present and easy to do. Continue rinsing. Seek medical attention if pain persists.
Skin contact: Wash with plenty of soap and water. If skin irritation or rash occurs: seek medical advice. Wash contaminated clothing before reuse.
Inhalation: If symptoms appear: move to fresh air and ventilate the suspected area.
Ingestion: Do NOT induce vomiting. If vomiting occurs spontaneously, keep head lower than hips. Transport to nearest medical facility.
5. FIREFIGHTING MEASURES
Suitable extinguishing media: Dry sand, CO₂, foam, dry powder.
Unsuitable extinguishing media: Strong water jet.
Hazardous combustion products: CO₂, CO, toxic pyrolysis products.
Firefighter protection: Use breathing apparatus, protective clothing, rubber boots, gloves.
6. ACCIDENTAL RELEASE MEASURES
Personal precautions: See section 8 for PPE. Wear protective clothing and gloves.
Emergency procedures: Absorb with inert absorbent material (sand, sawdust, silica gel).
Environmental precautions: Avoid discharge into the environment.
Cleanup methods: Clean up spills immediately using absorbent material. Collect waste in labeled containers per local regulations.
7. HANDLING AND STORAGE
Handling: Wash hands after handling. Ensure good ventilation. Comply with occupational exposure limits.
Storage: Cool, dry, well-ventilated area. Keep container closed. Keep away from heat/sunlight. Storage temperature: 5°C–35°C.
8. EXPOSURE CONTROLS/PERSONAL PROTECTION
Exposure limits: Not established.
Respiratory protection: Use organic vapor respirator if inhalation risk exists.
Eye protection: Wear splash goggles. Eyewash station nearby.
Skin protection: Wear impermeable gloves, protective clothing.
General: No eating/drinking/smoking at workplace.
9. PHYSICAL AND CHEMICAL PROPERTIES
	Property
	Value

	Physical state
	Liquid

	Color
	No data

	Odor
	Solvent odor

	pH
	Not applicable

	Melting point
	No data

	Boiling point
	No data

	Flammability
	Flammable liquid (flash point to be measured)

	Vapor pressure
	No data

	Relative density
	No data

	Solubility
	Insoluble in water

	Viscosity
	No data



10. STABILITY AND REACTIVITY
Stability: Stable under normal conditions and recommended storage.
Conditions to avoid: Heat and open flames.
Materials to avoid: Strong oxidizing agents, strong alkalis, strong acids.
Hazardous decomposition: CO, CO₂, and other organic compounds upon combustion or thermal decomposition.
11. TOXICOLOGICAL INFORMATION
	Endpoint
	Classification

	Acute skin irritation
	Not classified (may cause slight irritation)

	Acute eye irritation
	Not classified (may cause eye irritation)

	Respiratory sensitization
	Not classified

	Skin sensitisation
	May cause an allergic skin reaction (H317)

	Carcinogenicity
	May cause cancer (H350)

	Reproductive toxicity
	May damage the unborn child (H360D)

	STOT – single exposure
	May cause drowsiness or dizziness (H336)



12. ECOLOGICAL INFORMATION
Not classified as hazardous to the environment.
	Parameter
	Value

	Ecotoxicity
	Not classified

	Bioaccumulation
	None

	Persistence/degradability
	Alkyd resin degrades slowly; ester solvents are readily biodegradable



13. DISPOSAL CONSIDERATIONS
Dispose in accordance with official regulations. Do not pour into drains. Waste and packaging are hazardous waste.
14. TRANSPORT INFORMATION
Domestic/Sea/Air: UN 1263 – PAINT RELATED MATERIAL, Class 3 (flammable liquid), Packing group III.
15. REGULATORY INFORMATION
EU Regulations: Does not contain restricted REACH Annex XVII substances, REACH Candidate List substances, or REACH Annex XIV substances.
Product does not contain toxic heavy metals, free formaldehyde, azo compounds, phthalates, benzene. Complies with REACH, EN.71-3 (Europe), and CPSIA, ASTM (USA).
16. OTHER INFORMATION
Preparation date: 05/10/2026
The information describes safety requirements based on current knowledge. It is intended for safe handling, storage, processing, transport, and disposal of the product. Information does not necessarily apply to mixtures or processed materials.
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